The folder structure within this ZIP container is an image of the folders you will find in the original SES1.2.6 Software as provided from VG Scienta.

Copy all in this ZIP provided DLD files in your own SES folder following their position in this container. 

Note, that a new folder "SC_DLD" must be made with the provided files in it. 

The files "DLD.DLL" and "libtiff3.dll" must be copied in the SES root folder, that is the one where you find SES.EXE.

To make a DLD1818 simulation run, you may go to the new folder "SC_DLD" and rename the file "dld_gpx3_Make_Your_Own!.ini" into "dld_gpx3.ini".

Note, that your hardware will not be read in that simulation mode.

To work with your DLD hardware: check which DLD_GPG3.INI was delivered with your DLD package. 

You must copy your DLD_GPX3.INI into the new SC_DLD folder and your SES software will be ready to run with your DLD.

Check the DLD installation hints for DLDs in the provided DLD-SES overwiew sheet.

