This package contains an executable DLD-software version which runs without any hardware.

The simulation uses data which have be sampled with a DLD4444 by shining a 400nm laser onto different detector positions.

Just extract the included folder to any position on your computer.

You can run the either the DLD-monitor DLDGUI.EXE or the LabView-VI "LabViewDemo_DLD_LV8p2a.vi". 

(Note, that this demo runs in a special DLD raw data mode (G-Mode), which uses 8 pulse measurements per event from the DLD anode.
 This specialty can be seen in the behavior of the rate-meter, the 4 red DLD channel bars deliver double count rates for that mode unlike for the normal DLDs were all must be of about the same height.)

For LabView you must have installed LV version 8.2 or higher. 

Please start the "LabViewDemo_DLD_LV8p2a.vi" alway by double click in the Windows explorer, else LabView does not use the correct working path.

To work with your DLD hardware: check which DLD_GPG3.INI and which firmwarefile "*.RBT" was delivered with your DLD package. 
 
You must copy your DLD_GPX3.INI and your "*.RBT" into the folder of the DLD.DLL and your DLD software will be ready to run with your DLD.

Check the DLD installation hints for DLDs in the provided DLD-manuals.

